**Switch configuratie**

Building configuration...

Current configuration : 1373 bytes

version 15.0

no service timestamps log datetime msec

no service timestamps debug datetime msec

service password-encryption

hostname Switch1

enable secret WPL

spanning-tree mode pvst

spanning-tree extend system-id

interface FastEthernet0/1

interface FastEthernet0/2

interface FastEthernet0/3

interface FastEthernet0/4

interface FastEthernet0/5

interface FastEthernet0/6

interface FastEthernet0/7

interface FastEthernet0/8

interface FastEthernet0/9

interface FastEthernet0/10

interface FastEthernet0/11

interface FastEthernet0/12

interface FastEthernet0/13

interface FastEthernet0/14

interface FastEthernet0/15

interface FastEthernet0/16

interface FastEthernet0/17

interface FastEthernet0/18

interface FastEthernet0/19

interface FastEthernet0/20

interface FastEthernet0/21

interface FastEthernet0/22

interface FastEthernet0/23

interface FastEthernet0/24

interface GigabitEthernet0/1

interface GigabitEthernet0/2

interface Vlan1

description Switch1 to Router

ip address 192.168.1.2 255.255.255.0

ipv6 address 2001:DB8:1::2/64

banner motd ^CStay out access prohibited^C

line con 0

password WPL

login

line vty 0 4

password WPL

login local

transport input ssh

line vty 5 15

password WPL

login local

transport input ssh

end

**Router configuratie**

Building configuration...

Current configuration : 951 bytes

version 15.4

no service timestamps log datetime msec

no service timestamps debug datetime msec

service password-encryption

hostname Router

enable secret WPL

ip cef

no ipv6 cef

spanning-tree mode pvst

interface GigabitEthernet0/0/0

description connection to Switch1

ip address 192.168.1.1 255.255.255.0

duplex auto

speed auto

ipv6 address 2001:DB8:1::1/64

ipv6 address fe80::1 link-local

interface GigabitEthernet0/0/1

description connection to Switch2

ip address 192.168.2.1 255.255.255.0

duplex auto

speed auto

ipv6 address 2001:DB8:2::1/64

ipv6 address fe80::1 link-local

interface Vlan1

no ip address

shutdown

ip classless

ip flow-export version 9

banner motd #Stay out access prohibited#

line con 0

password WPL

login

line aux 0

line vty 0 4

password WPL

login local

transport input ssh

line vty 5 15

password WPL

login local

transport input ssh

end